|  |  |
| --- | --- |
| Firmware TO DO LIST (30-Jan-14) | DONE |
| * & (-) | X |
| * char / int8\_t sending temp data |  |
| * Mode fermentation: probe temp @ 10 sec / Mode brassage: probe temp @ 1 sec (tx to Brew\_Monitor mode) |  |
| * Au lieu send 0x9325 au debut, send reset ou « hello » to brew monitor |  |
| * Read UASRT AN |  |
| * Config XBee 1 channel, no broadcasting |  |
| * Test XBee signal? watchdog AND (LOST SIGNAL HANDLING) |  |
| * Checksum? |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |